**50 Scale Block Map Upgrade v1.1**

1. Removed Proposed Circuit Point layer
2. Shrunk Conductor Tie (Primary UG/Mesh) from size 4 to 2
3. Updated Antenna symbol to match ED Mapping
4. Removed Dimension, Duct Notes, Electric Splice, Electric Connector, Communication Splice, Communication Connector from UFM Group Layer
5. Added Wall to Floor Leader Line to UFM Group Layer
6. Changed Substation symbol color from red to black
7. Merged Overhead Pseudo Service layer into Secondary Overhead Conductor (removing Psuedo Service as a layer)
8. Merged Underground Pseudo Service layer into Secondary Underground Conductor (removing Psuedo Service as a layer)
9. Added DC Conductor 50 scale anno
10. Changed color of Conduit System from black to blue
11. Added cross section leader line layer to Conduit and Subsurface Structure