

**50 Scale Block Map Upgrade v1.2**



1. Shrunk Subsurface Structures’ Duct Junction subtype (“Enlosures” layer) from size 10 to size 5 (Repeat for proposed)

Before: After:



1. Modified Duct Bank symbology to include a black outline with white fill

Before: After:



 

1. Modified Duct symbology to use a solid black outline with a grey fill (20%) for occuplied and a solid white fill for unoccupied

Before:

After:

Upon completion:

